SAMPLE FOF MATERIALS

115 Laburnum Road, Hayes, Middlesex, UB3 4JZ

1. External Finish
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2. Roof Tiles

BMI Redland 49 30 Slate Grey (Smooth) 1101-30
[image: BMI Redland 49 30 Slate Grey (Smooth) 1101-30]
3. Windows

Top Opening Double Glazed Casement White UPVC Window
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SILICONE THIN COAT (TC)

Primer T

Slicone TC is a ready to use organic e Ihin Goal range is parlicularly sullasie whers Tghiweighl render
rasin render which Is appliac 1 provide Syslerns are requited, Such 25 an exeral wal suslon sysiem
a low maintenance textured fish. It is (ilustratod ool

avallatie i dilferent lexiures anc 2 wide
varioty of aclaurs. Prior 1o appicaton
Ine subsirale should be primed Using
Primer TG,

Reaquire:

Silicone TC 05 1.8kg / 5 1
Silicone TC 10: 1.8kg / 59 m aporex. 4 . o 163 o o
Silicono TC 15: 2.5 k& / 5 m approx

Silicons TC 80: 5.0 k5 / 5 M1 2pprox.

Product classification according to
BS EN 15824:2008

Goaling Malerisl DIN 18558 — P Org 1
A water-cilutable product for exteror
ancinierion Use
Water vapenr penmeabity - Category V2
Water absarpiion  Catogery W 3;
Achesion - 0.65 M3,
Themnal Goncetivity:

A 10, dry P-50%) - 0.8,

10, ey (P-80%) — 00

Reaction 1o fire - Class B-52.00
Product Classification (DIN 18558)
Cosling Materisl DIN 18552 - 1> Org 1

AL Golour Tustrarions shown in 1hia Hrochure &
s aceurate as tho printing procoss will alow. It s
Imporant thal & sampls 16 oblaine) 25 we reconimend
calours bo verified against K Mend Thin Goat sampes
befors orcer g,





image2.jpeg




image3.jpeg




