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This report is proposed to satisfy Planning Condition No 11, item c in relation to minimizing water use.  We would note the following;
This scheme has been designed to incorporate water saving measures and equipment as follows;

1. Water meters shall be provided on all CWS and DHWS systems to monitor water usage by the BMS. 

2. The BMS will provide leak detection and an early warning of any high water usage to the building operators.

3. Water shutoff valves shall be provided in each WC area to isolate the hot and cold water controlled by an occupancy sensor to avoid wastage caused by water leaks.

4. All WC’s shall be dual flush with 4/6 litre flushing options to minimise MCWS usage. This is only a small element of overall water usage.

5. Limited flow spray taps will be used to all washbasins to minimise water usage.

6. DHWS systems will have minimal dead legs to prevent water wastage.

7. The Science laboratories will have an independent isolated system to prevent back syphonage; only cold water will be used in Labs by students.

8. In the main kitchen and food technology rooms, all sinks shall be provided with suitable taps to minimise water wastage.

9. To avoid pupils wasting cold water in toilets, 10 No Chilled drinking water points shall be provided in various areas of the UTC.
Due to the design of the roof and modules and usage patterns of this Media specialist building, it is uneconomic and impractical to utilise a grey water system to serve the limited number of WC’s (which is only a small part of the water demand) and the design approach has targeted minimising water usage to all areas, catering, science, sports and general use.
