


1. Permeable paving area – “D” – INTERLOCKING BRICK PAVERS
            Reference: Site Investigation Report and Borehole/trial pit information.
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2. Non permeable surfacing  
· Proposed Building Roof has a foot print area 55sq.m
· Patio at the rear : 3.5 sq.m ; say a total of 60 sq.m – Non permeable area.
[bookmark: _GoBack]


· There is a fall towards a permeable area – Front and Rear Garden Area
· All roof downpipes connected straight into a pipe which flows onto the permeable area.
· Retain a permeable area within the front garden of 25%. This should be a sufficient Sustainable Drainage system such as sized soakaway, or flower bed, french drain, which would adequately manage and control the flow of surface water.
· A suitably sized collection system directing water towards the permeable front garden. This must not be connected to the mains drainage.
· Ensure there will be continual inspection and maintenance so that it is clear of debris.
image1.emf

