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                                     Fire Safety Statement






Consideration of the PFSS and has been considered in accordance with criteria of the London Plan Policy D12(A)
MEANS OF ESCAPE 
Where there is a means of escape from a first-floor level, this will not be compromised by the addition of an extension. Experience and time have shown the addition of an extension below a window is regarded, in the majority of instances, to aid a person’s evacuation or descent. 
As standard the glazing is manufactured with a maintenance loading – in effect this means consideration has been given to a person accessing the roof/glass – eg window cleaner, or as a fire escape in the event of an emergency 
A Guide to Good Practice in the Specification and Installation of Conservatories within the United Kingdom- Section 5.9.1’ April 2016 produced by The Glass and Glazing Federation state the following: “The roof covering and profiles need to be Class 1 rated to BS 476 part 7, (similarly AA rated to part 3-or classed TP(a) or TP(b) or BS 476:3 2004. There are compliant polycarbonates, glass products and profiles on the market”.
Other considerations
· Identify a suitably positioned unobstructed outside space for fire appliances to be positioned on:

The most suitable place would be on the highway to the front of the property 

· Provide suitable access and equipment for firefighting which is appropriate for the size and use of the development:

The proposal is for a minor development. Access and equipment will remain as the current situation

· Has the proposal been designed and considered in an appropriate way to minimise the risk of fire spread:

The proposed single storey structure and will remain low risk as there will be no cooking/sleeping facilities within the structure. 

image1.emf

