Surface Water Drainage and Flood Prevention 
6.16 Strategic Planning Guidance notes that unless carefully sited and designed, new development can exacerbate problems of flooding in areas downstream through an increase in run-off from additional roofs and paved surfaces. Boroughs are advised therefore, in association with the Environment Agency, to take into account in their UDPs the surface drainage consequences of new development, including the need to protect the flood plain and urban washlands (SPG, para 68). 

6.17 The Environment Agency has recently carried out extensive flood alleviation studies of the three principal watercourses in the Borough, the River Pinn, the River Colne catchment (including the River Frays, Duke of Northumberland River and the Grand Union Canal) and the River Crane catchment (including both arms of Yeading Brook). The aim of these studies is to remove the risk of regular flooding from existing development, and flood defence measures are being designed and implemented. However, in order that the risk of flooding is not increased elsewhere it is essential that the level of future development of the floodplain is strictly controlled, and that the capacity of the available flood plain is not reduced, or the flow of water impeded. The Local Planning Authority will have regard therefore to the drainage implications of new development and will liaise with the Environment Agency to ensure that proper provision is made. In particular the Local Planning Authority will have regard to the Environment Agency's advice on areas liable to flooding. 

OE7 IN THE AREAS LIABLE TO FLOODING PERMISSION WILL NOT BE GRANTED FOR NEW DEVELOPMENT OR THE INTENSIFICATION OF EXISTING DEVELOPMENT UNLESS A DEVELOPER IS PREPARED TO IMPLEMENT FLOOD PROTECTION MEASURES AS PART OF THE PROPOSED DEVELOPMENT TO A STANDARD SATISFACTORY TO THE COUNCIL, IN CONSULTATION WITH THE ENVIRONMENT AGENCY AND WHERE APPROPRIATE, OTHER DRAINAGE BODIES. 
OE8 PLANNING PERMISSION WILL NOT BE GRANTED FOR NEW DEVELOPMENT OR REDEVELOPMENT OF EXISTING URBAN AREAS WHICH WOULD RESULT IN AN INCREASED FLOOD RISK DUE TO ADDITIONAL SURFACE WATER RUN-OFF, UNLESS THE PROPOSED DEVELOPMENT INCLUDES APPROPRIATE ATTENUATION MEASURES TO A STANDARD SATISFACTORY TO THE COUNCIL, IN CONSULTATION WITH THE ENVIRONMENT AGENCY AND, WHERE APPROPRIATE, OTHER DRAINAGE BODIES. 
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