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1.0 Existing Site
Yeading Infant School is a mixed school for 3 to 7 year olds, with a current roll of 478 pupils.  
The majority of the school buildings date from the 1930’s, with a number of later extensions also provided.  The school kitchen and dining room is located to the rear of the school and has been identified as being an insufficient size for the needs of the school.

The existing Kitchen and Dining Room facilities are located within a detached single storey, post-war “Horsa” type concrete framed, prefabricated building. The building is located to the rear of the main buildings that form the school. The facility is provided with a dual pitched, timber framed main roof weathered with mineral felt. The external walls comprises pre-cast concrete panels and previously painted render.
The kitchen and dining room is provided with a solid concrete floor slab. Internally the property is provided with solid brick internal walls. The external walls have been provided with a plastered and painted wall finish. The ceiling comprises previously painted timber boarding. Timber, assumed load bearing posts are provided, where we assume there would have been originally an internal wall between the main part of the building and the section of building that protrudes to the east facing elevation.
Accommodation within the kitchen and dining room comprises of an open plan Dining Hall area with Staff Room and storage facilities to the east facing elevation. The property also is provided with a Kitchen, Dry Storage area and other associated facilities. Staff and pupil WC facilities are also provided.
Yeading Infant and Nursery School is not Listed, but it is, we understand, located within a Conservation Area.
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Photo. No. 1 Kitchen and Dining Room.
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Fig. No. 1 Kitchen and Dining Room Existing Plan
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Fig. No. 2 Kitchen and Dining Room Existing Site Plan

2.0
Proposed Development


The proposed works to be undertaken are as follows:-
1. The repair and extension of the existing kitchen/dining room.
There are two main rationale behind the proposed development, which are outlined in greater detail below:-
1. The Condition of the Existing Building

The existing building was constructed in the 1950’s and by its nature was considered to be a temporary building, with a limited lifespan.

The building is now over 70 years old and is not fit for purpose.  The thermal performance of the various different building elements is poor.  The building is not provided with a suitable space heating system.  The various external elements to the building are in a deteriorating condition having been extensively patch repaired in the past.
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Photo. No. 2. Example of External Condition of Building
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Photo. No. 3 Example of External Condition of Building
2. The Size of the Existing Building

The existing building is of insufficient size to properly cater for the schools requirements.  The capacity of the existing building allows for only approximately 60 pupils to sit at a time.No. pupils.  With a roll of over 450 pupils, this means there are multiple “sittings”, which has an adverse knock on implication in terms of teaching and delivery of the curriculum.
In order to address the above issues, it is proposed to carry out a major repair and extension of the existing building.
The building will be increased in size to approximately 350m².  This will increase the capacity of the dining hall area to approximately 150 pupils. This will allow for lunch service to be delivered in two sittings.
This will allow for lunch service to be undertaken in two sittings and reduce the adverse impact upon teaching.
In conjunction with the extension of the property the building will be repaired and refurbished.  This will include renewal of roof coverings, incorporating thermal insulation to the current standards, repair and upgrading of the external walls, again incorporating thermal insulation to current standards.  Other works proposed include renewal of the heating installation, new windows and doors and rainwater goods.

[image: image7.jpg]



Photo. No. 4 Existing Dining Room Area
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Fig. No. 3 Proposed Kitchen and Dining Room Plan with Seating Layout Added
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Fig. No. 4. Proposed Plan with Existing Plan Overlaid.
3.0 Proposed Materials
The building is to be provided with a “Britmet” Pantile 2000 lightweight steel core type roof cladding system to both the existing and new sections of the roof.
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Fig. No. 5. Example of Proposed Roofing Cladding System
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Fig. No. 6. Proposed Roof Cladding System
The new and existing external walls are to be provided with an “Eternit” Cedral Click smooth fibre cement type external weather board cladding system.  
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Photo. No. 5 Example of Cedral Cladding and Metal Powder Coated Windows.
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Photo. No. 6. Example of Metal Powder Coated Windows and Cedral Cladding System
The new doors and windows will be metal powder coated double glazed doors and windows. Refer to Photo Nos. 5 and 6.
4.0 Scale
The proposed works will not have any impact with regards to the existing mass or scale of the property.  The height of the extension will not exceed the existing height of the main buildings to the site.
5.0
Access

The proposed works do not have any impact on access to the property.   
6.0
Environment

Existing waste storage facilities are to be maintained and enhanced.
The proposed works do involve the removal of 2 No. existing mature trees.
The proposed works do not have any other environmental implications.

Working hours will be Monday to Friday 8.00am to 6.00pm and 9.00am to 1.00pm Saturday.  There will be no Sunday working.
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