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118 LARCH CRESCENT, HAYES, UB4 9EB
Specification for soft landscape works.
PLANTING:

MATERIALS

Trees and Shrubs:

Plant materials to be best quality nursery stock as specified in the schedule .
All plant materials shall conform to the minimum requirements of the following British Standard:  BS3936 – Nursery Stock.
The root-ball should be intact, firm and free from pernicious perennial weeds.

WORKMANSHIP

Setting Out:

Plants are to be positioned evenly and informally within each group, making allowance for overlapping of adjacent groups

Planting of Trees and Shrubs

Planting of shrubs shall be carried out between March and October 2017 avoiding periods of frost, drought or cold drying winds.  Holes should be dug of a sufficient size to take the undisturbed compost and root fibre of the container grown plants.
GRASS AREAS - TURFING
MATERIALS
Turf:

The turf shall be good quality meadow or downland turf, complying with the latest edition of BS3969, fibrous, well-rooted, mown and free from matted or dead grass of pernicious weeds, following treatment by selective weed killer not more than three months previously.

Individual turves to be 900mm x 300mm of regular size and not less than 25mm in even thickness throughout.

All turves to be obtained from approved sources.

Water:

Clean mains supply.  

WORKMANSHIP
Final Preparation of Soil:

Before laying the turf, bring the soil to an even tilth and necessary firmness and remove any large stones.  

 Laying Turf:

No turf shall be laid in exceptionally dry or frosty weather or in otherwise unsuitable weather conditions.

Turves to be laid in rows on the prepared soil bed, starting at one end of the area to be turfed and laid progressively by placing planks over the last row of turves laid and planks to be moved forward after each line of turves laid and so on to the end of area.

Turves to be laid half-lapped joints, well butted up and evenly beaten, twice over the whole area, with wooden turf beaters. The bottom of the wooden beaters to be frequently scraped clear of accumulated soil or mud.  

Any irregularities in finished levels, owing to variation in turf thickness or unequal consolidation of soil is to be adjusted after the first beating by raking and/or packing fine soil under turves to obtain an even surface for the while.

The finished levels of turf abutting paving must be not less than 25mm above the adjacent hard surfaces after laying and beating operations.
Watering:

On completion of turf laying the grass is to be thoroughly soaked with water to ensure establishment.

First Cut:

The grass is to be cut when it has grown to 70mm to half the original height and an approved lawn fertiliser is to be applied with a spreader at the rate of 70gm/m sqd.  All grass mowings and arisings are to be swept clean and removed from the ground.

Implementation Programme for Soft Landscape Works 

The soft landscape works are to be carried out in the first planting season after the completion of the building works, during the period from March to October 2017.
8.2   Details of hard landscaping:

8.2.a   Refuse storage is shown on drawing number 1034/60E as approved and received 19th   

           August 2013 (attached).

8.2.b   Means of enclosure/boundary treatments as shown on 1034/60E. 
The existing boundaries timber fencing will be retained and the new fencing will be of the same height as the existing installed to separate the gardens of the newly separated houses.
8.2.c   Hard Surfacing Materials – On the drawing number 1034/60E, parking spaces have been                                              

 shown and will constructed of permeable block paving marshall's priora color brindle..                                                                                                                                                 

Similarly, any paving in the rear gardens will be of the similar materials and colour and                      
will be permeable.
8.3 Details of Landscaping Maintenance:

8.3.a
A landscape gardener will be employed to carry out periodical maintenance and upkeep of the gardens and house fronts for a minimum period of 5 years.

8.3.b   Any trees or shrubs or area of turfing/seeding within the landscaping scheme which dies will be replaced with the same species.
The submitted Landscaping Scheme details will preserve and enhance the visual amenities of the new development, the locality providing adequate facilities in compliance with policies BE13, BE38 and AM14 Hillingdon Local Plan: Part Two Saved UDP Policies (November 2012).   
