The existing brick wall garden fence , runs 15 m along the entire width of the garden, and 6m from the rear left corner, 6m down length of the rear left side of the garden.  The length of the rear  garden is approximately 16 metres, and so it only runs partially along the left boundary.  The exiting wall is made up of red brick pillars with natural stone / beige colour wall in-between from breeze block material. The height of the highest point of the existing garden wall fence, is the pillars, which are 6ft.

Permission is sought to extend the fence up to 9ft at the highest point, by extending the brick pillar, currently 6ft, to 9ft high, and then add wooden fence panels inbetween which would sit on top of the existing breeze block brick wall.

The purpose of this is provide privacy, but also because the garages of the 3 properties that sit behind the rear garden, all extend far above the existing garden wall, which means our garden view is the back of unfinished, unrendered garage rear walls. 
The neighbour to the right (our semi detached neighbour) has an existing garden fence, partially brick, partially wooden panelling, which is 9ft. if planning permission were granted it would be in line with this fence also , so aesthetically, it would be consistent. 

The gardens which back on to the rear of our garden, where the garages are built, sit 2.5 feet above the level of our garden, and so the fence though 9ft on our side, would be 6.5 feet on their side.
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